Login/logout at the phone
*0 Extension	 Login user to phone. The PIN has to be entered and confirmed with the "#"-key.
*0*	 Logoff user from phone
Call Forwards
*2	 Activate call forwarding for calls from internal and external in case "always" to the default number. (A default number needs to be set in menu "Redirects"!)
*2 Number	 Activate temporary call forward for calls from internal and external in case "always" to the given number
*2#	 Program call forwarding for calls from internal and external in case "always". The destination needs to be entered and confirmed with the "#"-key.
*21	 Program call forward for calls from internal and external in case "always" to the voice mail.
*22	 Program call forward for calls from internal and external in case "always" to the voice mail announcement without mailbox.
*24	 Program call forward for calls from internal and external in case "always" to parallel call
*2*	 Deactivate call forwarding for calls from internal and external in case "always"
*90	 Activate call forwarding for calls from internal in case "always" to the default number. (A default number needs to be set in menu "Redirects"!)
*90 Number	 Activate temporary call forward for calls from internal in case "always" to the given number
*901	 Program call forward for calls from internal in case "always" to the voice mail.
*902	 Program call forward for calls from internal in case "always" to the voice mail announcement without mailbox.
*904	 Program call forward for calls from internal in case "always" to parallel call
*90*	 Deactivate call forwarding for calls from internal in case "always"
*91	 Activate call forwarding for calls from external in case "always" to the default number. (A default number needs to be set in menu "Redirects"!)
*91 Number	 Activate temporary call forward for calls from external in case "always" to the given number
*911	 Program call forward for calls from external in case "always" to the voice mail.
*912	 Program call forward for calls from external in case "always" to the voice mail announcement without mailbox.
*914	 Program call forward for calls from external in case "always" to parallel call
*91*	 Deactivate call forwarding for calls from external in case "always"
Call Waiting
*92	 Anklopfen aktivieren
*92*	 Anklopfen deaktivieren
Wakeup call
*40	 Set up a wakeup call
Pickup call
*81* Extension	 Directed pickup of calls
Check Voicemail
80	 Check own mailbox (on snom phones also possible by using the "Retrieve"-key)
80 Extension	 Check other mailbox (requires PIN)
Record unavailable message
*99*	 Record unavailable message for calls from internal
*98*	 Record unavailable message for calls from external
Queues
*5 Extension	 Login to the queue with given number
*5 Extension *	 Logout from the queue with given number
*5*	 Log out of all queues
Agents
*6 Agent number	 Direct login of an agent. The PIN has to be entered and confirmed with the "#"-key.
*6*	 Logout agent
*6#*	 Activate pause status for the agent
*6##	 Deactivate pause status for the agent
Conferences
88 Conf.no.	 Enter or create a conference room (dial 88, followed by an arbitrary 3 or 4 digits long number). If the conference room is empty, a PIN can be set up (for no PIN press #). If a PIN is already set up, it has to be entered to join the conference room.
88000 or 880000	 Find a free conference room. Will read out the conference number on joining.
Caller ID suppression (CLIR)
*31	 Caller ID suppression of own caller ID for the next internal or external call
*31*	 Deactivate caller ID suppression (internal and external)
*31Destination	 Suppression of the own caller ID for a call to an arbitrary destination
*32	 Permanent suppression of the own caller ID for all internal destinations
*32*	 Deactivate suppression of the own caller ID for all internal destinations
*33	 Permanent suppression of the own caller ID for all external destinations
*33*	 Deactivate suppression of the own caller ID for all external destinations
Displayed caller ID (CLIP)
*34	 Use the default as displayed caller ID for internal calls
*34Number	 Use the given number as displayed caller ID for internal calls
*35	 Use the default as displayed caller ID for external calls
*35Number	 Use the given number as displayed caller ID for external calls
*36Number	 Als angezeigte Rufnummer für das nächste interne Gespräch die angegebene Nummer festlegen
*37Number	 Als angezeigte Rufnummer für das nächste externe Gespräch die angegebene Nummer festlegen